# This file maps the raw RSSI values to dBm values to send to the DMR network. A number of data
# points should be entered and the software will use those to work out the in-between values.
#
# The format of the file is:
# Raw RSSI Value		dBm Value
#
# Measured with a Marconi 2955 Test set and Motorola GM340 UHF (430.6125 MHz) using Arduino DUE with ZUM v1.0.
# No resistor divider, 100nF decoupling capacitor from ADC to ground.
# Both S-meter (6dB) and decade (10dB) steps are included between the noise floor and saturation.
# George M1GEO / GB7KH - 01/01/2017
#
2858		-20
2857		-30
2856		-40
2855		-43
2854		-48
2853		-50
2845		-53
2780		-58
2732		-60
2647		-63
2484		-68
2422		-70
2356		-73
2234		-78
2183		-80
2103		-83
1978		-88
1931		-90
1875		-93
1710		-99
1686		-100
1545		-105
1416		-110
1398		-111
1238		-117
1166		-120
1106		-123
1018		-129
1006		-130
985		-135
976		-140
971		-150
